Практическое занятие №12 Управление сетевыми ресурсами и утилиты командной строки для работы с сетью.
Цель занятия:
Освоить базовые принципы и практические навыки настройки сетевых подключений, управления IP-адресами, а также диагностики сетевых соединений с помощью командной строки в операционной системе Debian.
Задачи занятия:
1. Познакомиться с основами сетевых подключений и компонентами сети в Debian/Linux.
2. Научиться настраивать статический и динамический IP-адрес с использованием конфигурационных файлов.
3. Освоить работу с основными сетевыми конфигурационными файлами Debian: /etc/network/interfaces и /etc/network/interfaces.d/.
4. Научиться диагностировать и тестировать сетевые подключения с помощью утилит командной строки: ping, traceroute (или tracert), netstat.
5. Познакомиться с основными сетевыми сервисами Debian: Apache2, BIND9, ISC-DHCP-Server, их назначением и ролью в управлении сетью.
План занятия:
Часть 1: Основы сетевых подключений на Debian
1. Обсуждение, что такое сетевое подключение и его основные компоненты: сетевые адаптеры, кабели, маршрутизаторы.
2. Типы подключений: проводные (Ethernet) и беспроводные (Wi-Fi).
Часть 2: Настройка сети на Debian
1. Обзор конфигурационных файлов /etc/network/interfaces и /etc/network/interfaces.d/.
2. Практическая работа с текстовым редактором (например, nano или vim): открытие и редактирование файла конфигурации сети.
Часть 3: Настройка статического IP-адреса
1. Понятие статического IP и его назначение.
2. Практическое задание: прописать параметры интерфейса (IP-адрес, маска, шлюз) в конфигурационном файле, применить изменения, перезапустить сетевые службы.
Часть 4: Настройка динамического IP-адреса через DHCP
1. Понятие динамического IP и роль DHCP.
2. Установка и настройка DHCP-клиента.
3. Конфигурация получения IP по DHCP, перезапуск служб.
Часть 5: Диагностика и тестирование сетевых соединений
1. Использование команд:
1. ping — проверка доступности хоста.
2. traceroute — отслеживание маршрута до узла.
3. netstat — анализ текущих сетевых соединений и портов.
2. Практические примеры и разбор результатов.
Часть 6: Основные сетевые сервисы Debian
1. Краткий обзор и назначение:
1. Apache2 — веб-сервер.
2. BIND9 — DNS-сервер.
3. ISC-DHCP-Server — DHCP-сервер.
2. Роль и значение для управления сетевыми ресурсами.
Итог: Обсуждение вопросов, разбор типичных ошибок при настройке сети, рекомендации по дальнейшему изучению.
Теоретическая часть
1. Основы сетевых подключений в Debian/Linux
Что такое сетевое подключение?
Сетевое подключение — это механизм, позволяющий устройствам обмениваться данными друг с другом через сеть. В операционных системах Linux, таких как Debian, сеть обеспечивает взаимодействие как внутри локальной сети, так и с внешними ресурсами.
Компоненты сетевого подключения:
1. Сетевые адаптеры (Network Interface Cards, NICs): физические или виртуальные устройства, обеспечивающие доступ компьютера к сети.
2. Кабели и разъемы: для проводных соединений (например, Ethernet-кабели).
3. Маршрутизаторы и коммутаторы: устройства, которые управляют передачей данных между узлами сети.
Типы сетевых подключений:
1. Проводные (Ethernet): надежные, обеспечивают высокую скорость передачи данных.
2. Беспроводные (Wi-Fi): удобны для мобильных устройств, обеспечивают гибкость, но могут иметь ограничения по скорости и стабильности.
2. Настройка сети в Debian/Linux
В Debian настройка сети производится через системные конфигурационные файлы. Основные из них — это:
1. /etc/network/interfaces
2. Каталог /etc/network/interfaces.d/
В этих файлах задаются параметры для сетевых интерфейсов, такие как IP-адрес, маска подсети, шлюз по умолчанию и прочие параметры.
Для редактирования этих файлов используются текстовые редакторы (nano, vim, gedit и др.).
3. Статический и динамический IP-адрес
Статический IP-адрес — постоянный адрес, который назначается устройству вручную. Используется для серверов, принтеров и других устройств, которым требуется постоянный адрес в сети.
Настройка статического IP включает указание:
1. IP-адреса
2. Маски подсети
3. Основного шлюза (gateway)
4. DNS-серверов (если нужно)
Динамический IP-адрес — адрес, который автоматически присваивается устройству через DHCP-сервер. DHCP (Dynamic Host Configuration Protocol) упрощает управление сетью, автоматически распределяя адреса и другие параметры.
4. Диагностика и тестирование сетевых соединений
Для диагностики и анализа состояния сети в Linux широко применяются следующие команды:
1. ping — проверяет доступность удаленного узла, отправляя ICMP-запросы. Помогает определить, отвечает ли хост, и измерить задержку.
2. traceroute — отображает путь, по которому проходят пакеты до указанного узла, показывая промежуточные маршрутизаторы. Позволяет выявить узкие места на маршруте.
3. netstat — выводит список активных сетевых соединений, открытых портов и используемых протоколов. Используется для анализа сетевой активности и выявления подозрительных подключений.
5. Основные сетевые сервисы в Debian/Linux
1. Apache 2 — популярный веб-сервер, позволяющий обслуживать веб-страницы и приложения. Поддерживает множество функций: виртуальные хосты, SSL, аутентификацию и др.
2. BIND9 — DNS-сервер, осуществляющий преобразование доменных имен в IP-адреса и обратно. Необходим для работы сети и интернета.
3. ISC-DHCP-Server — сервер DHCP, автоматически назначающий IP-адреса и сетевые параметры клиентам в сети, упрощая управление адресным пространством.
Итоги
Понимание принципов сетевых подключений и умение работать с конфигурационными файлами и диагностическими утилитами являются ключевыми навыками системного администратора. Настройка IP-адресов (статических и динамических), а также умение проверять состояние сети с помощью командной строки позволяют эффективно управлять сетевыми ресурсами в Debian/Linux.
Практическая часть
Для настройке сети мы воспользуемся второстепенной машиной , в которой у нас будет только консоль.
Ее устанавливать не надо, она уже собранна, достаточно ее просто запустить, логин и пароль oper, если права суперпользователя то root

В запущенной машине логинимся под root

Далее обновим и установим пакеты не обходимые для настройки сети

Вписываем пакеты для настройки сетевой части ,чтоб мы могли их использовать

И ждем конца установки пакетов


Выключаем полностью нашу машину
Теперь заходим в настройки машины,чтоб мы могли установить изолировать нашу машину от другим машин сделав из нее мини сервер выбирая Внутренняя сеть. После чего запускаем ее

Логинимся под root и проверяем наш сетевой интерфейс с помощью команды ip addr.

Система во втором интерфейсе по протоколу DHCP пыталась получить от вирутал бокса свой айпи , но мы изолировали и теперь сами настроем свою сеть.

Используем команду nano /etc/network/interfaces и переходим к редактированию нашего сетевого файла

Тут хранятся параметры наших сетевых карт, и нашу видим мы получаем по ней автоматический айпи, теперь сделай статический айпи и пропишем миниму параметров.

После чего сохраняем файл нажимая ctrl+o и выход из файла ctrl+x и перезапустим систему командой systemctl restart networking.service данной командой мы перезапускаем нашу сеть теперь используем команду ip addr и видим нашу измененную сеть.

И пропингуем свой же айпишник что проверить работу.

Теперь давайте настроем наш веб сервер через apache2, проверим каталог рута 

Сами каталоги настройки аpache2 находится по пути ls /etc/apache2/

Нас интересуют два конфигурационных файла наших сайтов, переходим в sites-available

С помощью команды ls видим два файла один для настроек http другой для https, давайте создадим свой вирутальный хост пишем nano na3.ex.conf и пропишем в нем минимальный набор строк для вирутального хоста

Тут мы даем ему имя, почта админа для связи и расположение нашего конфига, после чего сохраняем и закрываем, мы указали где лежит наш файл,но каталога такого нет, давайте его создадим

Второй командой мы проверяем создался ли каталог, теперь перейдем и посмотрим где наш конфиг

Теперь включим наш конфиг

Все окей, но теперь система просит перезапустить на apache2 , тут делема есть reload , а есть restart. Второй он полностью вырубает систему и останавливает процесс, но если сайт у нас работает 24 на 7 то пользователи не смогут попасть на данный сайт, reload он перезагружает на горячую и подключает новые конфиги, то есть не отрубается система, но если конфиги написаны с ошибками то они просто не запуститься. Пропишем reload

Теперь проверим наши две папки конфига Появился ли в нах наш конфиг 
Теперь если мы запустим наш файл  lynx na3.ex, то он выдаст ошибку

Ошибка означает , что не настроен DNS , но мы его сейчас обойдем чтоб проверить

Добавляем в файл третью строчку
Сохраняем и закрываем файл и повторяем команду lynx na3.ex
И видим индексовую заглушку так как файлов у нас там нет

Можно туда что-то добавить, чтоб проверить, к примеру текстовый файл 

Ну и заходя по новой снова увидим наш индекс и файлик

Теперь давайте настроем DNS с помощью пакета bind9 впишем команду nano /etc/hosts. В этом файле сделаем теперь правильную настройку, в тот раз мы сделали доступ к сайту для одного устройства, предположим у нас закрытый корпоративный сайт для 500 сотрудников, и мы должны настроить данную историю.  Чтоб нам прикрепить 500 компов, надо будет ходить по всем компам и в ручную всю настраивать, а это не удобно, закоментим ту строчку и сохраним

Далее сделаем чтоб наша машина понимала, что она DNS сервер пишем nano /etc/resolf.conf в файле вместо айпишника которого система нам при запуске выдала впишем наш статический.

Сохраняем , а теперь переходим к основной сложной части.
Переходим в каталог bind

Тут мы будем какие то файлы редактировать, а какие то добавлять. Начнем с этого


Тут создадим контроль доступа acl и даем ей имя после указываем разрешенный диапазон адресов , после ставим наш айпи локального хоста добавим перенаправление на днс 4-ри восьмерки.
 Добавим листен-он , она позволит слушать машины на определнном сетевом адаптерах

Сохраняем файл и проверим нет ли у нас ошибки в наших конфигурационных файлах
И видим у нас ошибки, давайте вернемся в тот файл и исправим

Ставим точки с  запятой 


И проверяем на ошибки, ошибок нет, всегда настраивая файл проверяйте его на ошибки, так как дальше у нас много файлов будет, проверив бы все после настройки всех, мы бы запутались, дальше идем в файл nano named.conf.local
 Тут мы пропишем зоны доступа к примеру к чему мы можем подключаться к яндексу гуглу и.т.д
Зона первого уровня будет главная и прописываем путь к данной зоне, она ьудет преобразовывать зону в айпишник , создадим обратную зоную. Создаем две зоны и проверяем на ошибки

Дальше у нас есть файлик , который нужно редактировать , но он очень большой
Теперь ,что мы сделаем мы скопируем командой его и дадим ему название и отредактируем






Ниже TTL это время жизни в секундах, добавим ORIGIN название нашей зоны и в конце ставим точку после ex. В сериал добавим дату сегодняшнюю и единицу, единица это номер правки нашего хоста,чтоб мы могли отслеживать и искать его как в базе данных. 
Теперь в NS-name server дадим имя , указываем запись а адрес наш айпи, удаляем айпи в 6 и пропишем наши хосты.

Теперь что мы делаем, мы скопируем данный файл , чтоб настроить обратную зону

Теперь откроем rz и отредактируем его

И теперь перезагружает bind9

Ошибок нет и проверим статус , вместо рестарт вписать статус и увидим зеленый глаз, значит dns работает

И с помощью команды checkconf -z проверим все наши зоны

Если бы была ошибка нам бы писалось следующие

Теперь применим все изменения командой rndc reload и пропингуем

Теперь настроем DHCP
Мы пакет для него в начале скачали,но сейчас он не активен и завален всяким хламом, система не понимает , что ей делать для этого мы можем проверить статус

Первым надо сделать на каком интерфейсе наш DHCP будет работать, для этого воспользуемся ip addr  возьмем второй интерфейс, так как DHCP должен работать на статическом ip

Далее редачим файл DHCP

У нас свободно две строчки , на какой из интерфейсов работать , закоментим ipv6, а в ipv4 пишем enp0s3

Сохраняем и идем в другой файл


Тут не торопимся и внимательно все делаем, коментим общие настройки , они нам не нужны

Теперь раскоментим авторетатив, так как он будет у нас самым главным в нашей сети и система будет обращаться к нему.

Теперь раскоментим журнал,любое событие к примеру что то случилось на сервере будет идти запись в журнал, кто то подключился к нашей сети . мы выдали ему ip сделали запись в журнал

Теперь как мы будем выдавать адреса, их там написано много от легко к простому воспользуемся базовым и раскоментим его и поменяем его на свою сеть и допишем имя сервера

Ниже исправленный как должно быть

И сохраняем, и перезапускаем систему командой

И проверим статус, рестарт меняем на статус и видим , что DHCP поднялся и работает

К примеру если мы подключим на виртуалке виндоус систему,главное , чтоб сетка у нее тоже была выбрана внутренняя сеть и мы можем проверить ip на сетевом адаптере и проверить сайт апача.



Вопросы для контроля знаний
1. Что такое сетевое подключение и какие основные компоненты входят в его состав?
2. Какие типы сетевых подключений существуют? В чем их основные отличия?
3. Какие конфигурационные файлы используются в Debian для настройки сети?
4. Как настроить статический IP-адрес на Debian? Какие параметры необходимо указать?
5. Что такое динамический IP-адрес и как он настраивается в Debian?
6. Какой протокол отвечает за автоматическую выдачу IP-адресов в сети?
7. Для чего используется команда ping? Как интерпретировать ее результаты?
8. Как с помощью traceroute можно диагностировать проблемы с маршрутизацией?
9. Какие сведения можно получить с помощью команды netstat?
10. Какова роль сервера Apache2 в сетевой инфраструктуре Debian?
11. Для чего используется DNS-сервер BIND9?
12. Какие функции выполняет ISC-DHCP-Server?
13. Какие шаги необходимо выполнить для применения изменений в сетевой конфигурации Debian?
14. Чем полезна работа с утилитами командной строки для администрирования сети?
15. Как можно проверить текущие сетевые интерфейсы и их состояние в Debian?
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root@debian:“# systemctl status isc-dhcp-server.service
« isc-dhcp-server.service - LSB: DHCP server
Loaded: loaded (/etc/init.dsisc-dhep-server; generated

Active: failed (Result: exit-code) since Sun 2024-02-18 18:46:29 MSK; 2min 5s ago
Docs: man:systemd-sysv-generator (8.
Process: 447 ExecStart=/etc/init.d/isc-ohep-server start (codesexited, status=1/FAILURE
CPU: T5ms
fee 18 :27 debian dhcpd [476] ¢ bugs on either our web page at wwu.isc.org or in the README file
tes 18 27 debian dhcpd[476] : before submitting a bug. These pages explain the proper
fee 18 :27 debian dhcpd [476] ¢ process and the information we find helpful for debugging
fee 18 :27 debian dhcpd [476] ¢
fee 18 :27 debian dhcpd [476]: exiting
fee 18 29 debian isc-chcp-server[447]: Starting ISC DHOPvd server: dhepdcheck syslog for diag
tes 18 29 debian isc-dhcp-server[447]:  failed
bes 18 29 debian sustend[1]: isc-dhcp-server.service: Control process exited, codesexited, st
fee 18 29 debian systemd(1]: isc-dhcp-server.service: Falled with result 'exit-code’

bes 18 18:46:29 debian systemd[1]: Failed to start isc-dhcp-server.service - LSB: DHCP server

rootadebian:“# ip addr

¢ 1o: <LOOPBACK,UP,LOMER_UP> mtu 65536 qdisc nogueue state UNKNOWN group default glen 1000
Link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo

\ valid_Lft forever preferred_lft forever
i

neté ::17128 scope host nopref ixroute
valid_Lft forever preferred_lft forever
enpos3: <BROADCAST, MULTICAST,UP,LONER_UP> mtu 1508 qdisc fq_codel state UP group default glen 100

Link/ether 08:00:27:6h:6e:3a brd ffff:ffiffffiff
inet 192.168.10.1/24 brd 192.168.10.255 scope global enposd
valid_Lft forcguerpreferred_Lft forever
inet fedo0::a00:2 6h:6e3a/64 scope Link
valid_Lft forever erred_Lft forever
root@dehian: “#
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root@debian:“# systemctl status isc-dhcp-server.service
« isc-dhcp-server.service - LSB: DHCP server
Loaded: loaded (/etc/init.dsisc-dhep-server; generated

Active: failed (Result: exit-code) since Sun 2024-02-18 18:46:29 MSK; 2min 5s ago
Docs: man:systemd-sysv-generator (8.
Process: 447 ExecStart=/etc/init.d/isc-ohep-server start (codesexited, status=1/FAILURE
CPU: T5ms
fee 18 :27 debian dhcpd [476] ¢ bugs on either our web page at wwu.isc.org or in the README file
tes 18 27 debian dhcpd[476] : before submitting a bug. These pages explain the proper
fee 18 :27 debian dhcpd [476] ¢ process and the information we find helpful for debugging
fee 18 :27 debian dhcpd [476] ¢
fee 18 :27 debian dhcpd [476]: exiting
fee 18 29 debian isc-chcp-server[447]: Starting ISC DHOPvd server: dhepdcheck syslog for diag
tes 18 29 debian isc-dhcp-server[447]:  failed
bes 18 29 debian sustend[1]: isc-dhcp-server.service: Control process exited, codesexited, st
fee 18 29 debian systemd(1]: isc-dhcp-server.service: Falled with result 'exit-code’

bes 18 18:46:29 debian systemd[1]: Failed to start isc-dhcp-server.service - LSB: DHCP server

rootadebian:“# ip addr

¢ 1o: <LOOPBACK,UP,LOMER_UP> mtu 65536 qdisc nogueue state UNKNOWN group default glen 1000
Link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo

\ valid_Lft forever preferred_lft forever
i

neté ::17128 scope host nopref ixroute
valid_Lft forever preferred_lft forever
enpos3: <BROADCAST, MULTICAST,UP,LONER_UP> mtu 1508 qdisc fq_codel state UP group default glen 100

Link/ether 08:00:27:6h:6e:3a brd ffff:ffiffffiff
inet 192.168.10.1/24 brd 192.168.10.255 scope global enposd
valid_Lft forcguerpreferred_Lft forever
inet fedo0::a00:2 6h:6e3a/64 scope Link
valid_Lft forever erred_Lft forever
root@dehian: “#
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‘¥ nano /etc/default/isc-dhen-server
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‘¥ nano /etc/default/isc-dhen-server
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¥ Defaults for isc-dhep-server (sourced by /etcsinit.dsisc-dhep-server)

 Path to dhepd's config file (default: setc/dhep/dhepd.conf)
DHCPDV4_CONF=/etc/dhen/dhepd . conf
DHCPDVE_CONF=/etc/dhcp/dhcpd . conf

¢ Path to dhepd's PID file (default: /var/runsdhepd.pid)
DHCPDV4_PID=/var/run/dhcpd . pid
DHCPDVE_PID=/var/run/dhcpdé . pid

¢+ Additional options to start dhepd with
' Don't use options -cf or -pf here; use DHCPD_CONF/ DHCPD_PID instead
0PTIONS="

! On what interfaces should the DHCP server (dhcpd) serve DHCP reguests?
' Separate multiple interfaces with spaces, e.g. “ethe eth1”

INTERFACESY4="enpos3"
INTERFACESVE="" &
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¥ Defaults for isc-dhep-server (sourced by /etcsinit.dsisc-dhep-server)

 Path to dhepd's config file (default: setc/dhep/dhepd.conf)
DHCPDV4_CONF=/etc/dhen/dhepd . conf
DHCPDVE_CONF=/etc/dhcp/dhcpd . conf

¢ Path to dhepd's PID file (default: /var/runsdhepd.pid)
DHCPDV4_PID=/var/run/dhcpd . pid
DHCPDVE_PID=/var/run/dhcpdé . pid

¢+ Additional options to start dhepd with
' Don't use options -cf or -pf here; use DHCPD_CONF/ DHCPD_PID instead
0PTIONS="

! On what interfaces should the DHCP server (dhcpd) serve DHCP reguests?
' Separate multiple interfaces with spaces, e.g. “ethe eth1”

INTERFACESY4="enpos3"
INTERFACESVE="" &
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rootedebian:™# nano etc/dhcp/dhepd. conf é
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rootedebian:™# nano etc/dhcp/dhepd. conf é
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# dhepd. conf
]

# Sample configuration file for ISC dhcpd
¢

# option definitions common to all supported netuorks. ..
option domain-name “example.org”
option domain-name-servers nsi.example.org, ns2.example.org;

default-lease-tine 600;
max- lease-time 7200;

# The ddns-updates-style paraneter controls whether or not the server will
# attenpt to do a ONS update when a lease is confirmed. We default to the
# behavior of the version 2 packages ('none', since DHCP v2 didn't

# have support for DDNS.)

ddns-update-style none;

# If this DHCP server is the official DHCP server for the local
# netuork, the authoritative directive should be uncommented.
#authoritative;

# Use this to send dhcp log messages to a different log file (you also
¥ have to hack syslog.conf to complete the redirection)
#log-facility locall;

# No service will be given on this subnet, but declaring it helps the
# DHCP server to understand the network topology.

#subnet 10.152.187.0 netmask 255.255.255.0 {
#

# This is a very basic subnet declaration

3anucats Touck
UnTiain amera

OTMEHa
ToeTop

Crpaska
BbiX0A

Bbipesars
il 6crasuTe

BHNOAHNTE Tosnuus
BPOBHATL K cTpoke





image511.png
# dhepd. conf
]

# Sample configuration file for ISC dhcpd
¢

# option definitions common to all supported netuorks. ..
option domain-name “example.org”
option domain-name-servers nsi.example.org, ns2.example.org;

default-lease-tine 600;
max- lease-time 7200;

# The ddns-updates-style paraneter controls whether or not the server will
# attenpt to do a ONS update when a lease is confirmed. We default to the
# behavior of the version 2 packages ('none', since DHCP v2 didn't

# have support for DDNS.)

ddns-update-style none;

# If this DHCP server is the official DHCP server for the local
# netuork, the authoritative directive should be uncommented.
#authoritative;

# Use this to send dhcp log messages to a different log file (you also
¥ have to hack syslog.conf to complete the redirection)
#log-facility locall;

# No service will be given on this subnet, but declaring it helps the
# DHCP server to understand the network topology.

#subnet 10.152.187.0 netmask 255.255.255.0 {
#

# This is a very basic subnet declaration
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Debian GNU/Linux 12 debian ttyl

debian login: root
Password:
Linux debian 6.1.0-13-amd64 #1 SMP PREEMPT_DYNAMIC Debian 6.1.55-1 (2023-03-29)

The programs included with the Debian GNU/Linux system are free sof tuare;
the exact distribution terms for each program are described in the
individual files in /usr/share/doc/x/copyright.

Debian GNU/Linux comes with ABSOLUTELY NO WARRANTY, to the extent
permitted by applicable law.
rootadebian:™¥ _
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# dhcpd. conf

a

# sample configuration file for ISC dhcpd
#

# Aﬂ()nn definitions common to all supported networks. ..
#option domain-name “example.org”
#option domain-name-servers nsi.example.org, ns2.example.org

default-lease-tine 600;
max- lease-tine 7200;

# The ddns-updates-style parameter controls uhether or not the server will
# attenpt to do a DNS update when a lease is confirmed. We default to the
# behavior of the version 2 packages ('none', since DHCP ve didn't

# have support for DONS.)

dens-update-style none;

# If this DHCP server is the official DHCP server for the local
# network, the authoritative directive should be uncommented.
wauthoritative;

# Use this to send dhcp log messages to a different log file (you also
# have to hack syslog.conf to complete the redirection)
#log-facility local;

# No service will be given on this subnet, but declaring it helps the
# DHCP server to understand the network topology.

#subnet 10.152.187.0 netmask 255.255.255.0
"t

# This is a very basic subnet declaration.
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# dhcpd. conf

a

# sample configuration file for ISC dhcpd
#

# Aﬂ()nn definitions common to all supported networks. ..
#option domain-name “example.org”
#option domain-name-servers nsi.example.org, ns2.example.org

default-lease-tine 600;
max- lease-tine 7200;

# The ddns-updates-style parameter controls uhether or not the server will
# attenpt to do a DNS update when a lease is confirmed. We default to the
# behavior of the version 2 packages ('none', since DHCP ve didn't

# have support for DONS.)

dens-update-style none;

# If this DHCP server is the official DHCP server for the local
# network, the authoritative directive should be uncommented.
wauthoritative;

# Use this to send dhcp log messages to a different log file (you also
# have to hack syslog.conf to complete the redirection)
#log-facility local;

# No service will be given on this subnet, but declaring it helps the
# DHCP server to understand the network topology.

#subnet 10.152.187.0 netmask 255.255.255.0
"t

# This is a very basic subnet declaration.
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# dhcpd. conf
a

# sample configuration file for ISC dhcpd
#

# option definitions common to all supported networks...
#option domain-name “example.org”;
#option domain-name-servers nsi.example.org, ns2.example.org;

default-lease-tine 600;
max- lease-tine 7200;

# The ddns-updates-style parameter controls uhether or not the server will
# attenpt to do a DNS update when a lease is confirmed. We default to the
# behavior of the version 2 packages ('none', since DHCP ve didn't

# have support for DONS.)

dens-update-style none;

# If this DHCP server is the official DHCP server for the local
# network, the authoritative directive should be uncommented.
authoritative;

# Use this end dhep log messages to a different log file (you also
yslog.conf to complete the redirection).
#log-facility INal7;

# No service will Be given on this subnet, but declaring it helps the
# DHCP server to understand the network topology.

#subnet 10.152.187.0 netmask 255.255.255.0
"t

# This is a very basic subnet declaration.
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# dhcpd. conf
a

# sample configuration file for ISC dhcpd
#

# option definitions common to all supported networks...
#option domain-name “example.org”;
#option domain-name-servers nsi.example.org, ns2.example.org;

default-lease-tine 600;
max- lease-tine 7200;

# The ddns-updates-style parameter controls uhether or not the server will
# attenpt to do a DNS update when a lease is confirmed. We default to the
# behavior of the version 2 packages ('none', since DHCP ve didn't

# have support for DONS.)

dens-update-style none;

# If this DHCP server is the official DHCP server for the local
# network, the authoritative directive should be uncommented.
authoritative;

# Use this end dhep log messages to a different log file (you also
yslog.conf to complete the redirection).
#log-facility INal7;

# No service will Be given on this subnet, but declaring it helps the
# DHCP server to understand the network topology.

#subnet 10.152.187.0 netmask 255.255.255.0
"t

# This is a very basic subnet declaration.
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# dhcpd. conf
a

# sample configuration file for ISC dhcpd
#

# option definitions common to all supported networks...
#option domain-name “example.org”
#option domain-name-servers nsi.example.org, ns2.example.org

default-lease-tine 600;
max- lease-tine 7200;

# The ddns-updates-style parameter controls uhether or not the server will
# attenpt to do a DNS update when a lease is confirmed. We default to the
# behavior of the version 2 packages ('none', since DHCP ve didn't

# have support for DONS.)

dens-update-style none;

# If this DHCP server is the official DHCP server for the local
# network, the authoritative directive should be uncommented
authoritative;

# Use this to send
# have to hack sysl
log-facility locall;

log messages to a different log file (you also
onf to complete the redirection)

# No service will be given on this subnet, but declaring it helps the
# DHCP server to understand the network topology.

[#subnet 10.152.187.0 netmask 255.255.255.0
"t

# This is a very basic subnet declaration.
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# dhcpd. conf
a

# sample configuration file for ISC dhcpd
#

# option definitions common to all supported networks...
#option domain-name “example.org”
#option domain-name-servers nsi.example.org, ns2.example.org

default-lease-tine 600;
max- lease-tine 7200;

# The ddns-updates-style parameter controls uhether or not the server will
# attenpt to do a DNS update when a lease is confirmed. We default to the
# behavior of the version 2 packages ('none', since DHCP ve didn't

# have support for DONS.)

dens-update-style none;

# If this DHCP server is the official DHCP server for the local
# network, the authoritative directive should be uncommented
authoritative;

# Use this to send
# have to hack sysl
log-facility locall;

log messages to a different log file (you also
onf to complete the redirection)

# No service will be given on this subnet, but declaring it helps the
# DHCP server to understand the network topology.

[#subnet 10.152.187.0 netmask 255.255.255.0
"t

# This is a very basic subnet declaration.
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default-lease-tine 600;
max- lease-tine 7200;

# The ddns-updates-style parameter controls uhether or not the server will
# attempt to do a DNS update when a lease is confirmed. We default to the
# behavior of the version 2 packages ('none', since DHCP ve didn't

# have support for DONS.)

dens-update-style none;

# If this DHCP server is the official DHCP server for the local
# network, the authoritative directive should be uncommented.
authoritat ive;

# Use this to send dhcp log messages to a different log file (you also
# have to hack syslog.conf to complete the redirection)
log-facility local?;

# No service will be given on this subnet, but declaring it helps the
# DHCP server to understand the network topology.

#subnet 10.152.187.0 netmask 255.255.255.0
"t

# This is a very basic subnet declaration.

subnet 10.254.239.0 netmask 255.255.255.224 {
range 10.254.239.10 10.254.239.20;
option routers rtr-239-6-1.example.org, rir-239-0-2.example.org;

13

# This declaration allows BOOTP clients to get dunamic addresses
# uhich we don't really recommend.
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default-lease-tine 600;
max- lease-tine 7200;

# The ddns-updates-style parameter controls uhether or not the server will
# attempt to do a DNS update when a lease is confirmed. We default to the
# behavior of the version 2 packages ('none', since DHCP ve didn't

# have support for DONS.)

dens-update-style none;

# If this DHCP server is the official DHCP server for the local
# network, the authoritative directive should be uncommented.
authoritat ive;

# Use this to send dhcp log messages to a different log file (you also
# have to hack syslog.conf to complete the redirection)
log-facility local?;

# No service will be given on this subnet, but declaring it helps the
# DHCP server to understand the network topology.

#subnet 10.152.187.0 netmask 255.255.255.0
"t

# This is a very basic subnet declaration.

subnet 10.254.239.0 netmask 255.255.255.224 {
range 10.254.239.10 10.254.239.20;
option routers rtr-239-6-1.example.org, rir-239-0-2.example.org;

13

# This declaration allows BOOTP clients to get dunamic addresses
# uhich we don't really recommend.

OTHEHa
ToBTOp

Crpaska
BbIXOA

3anucats Touck Bbpesats BHINOAHATE Tosnuus
YaTdann JaMeHa BCTaBUTL BHPOBHATE K cTpoke





image56.png
subnet 192.168.10.0 netmask 255.255.255.0 {
range 192.168.10.10 192.168.10.20;
optlon routers 192.168.10.

| option domain-name-servers 192.168.10.1;
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subnet 192.168.10.0 netmask 255.255.255.0 {
range 192.168.10.10 192.168.10.20;
optlon routers 192.168.10.

| option domain-name-servers 192.168.10.1;





image3.png
Debian GNU/Linux 12 debian ttyl

debian login: root
Passuord:
Linux debian 6.1.0-13-anded #1 SMP PREEMPT_DYNAMIC Debian 6.1.55-1 (2023-09-29) x86_64

The programs included with the Debian GNU/Linux sustem are free softuare;
the exact distribution terms for each program are described in the
individual files in /usr/share/doc/«/copuright.

Debian GNU/Linux comes with ABSOLUTELY NO HARRANTY, to the extent
permitted by applicable law.
root@dehian:“# apt update
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# This declaration allows BOOTP clients to get dynamic addresses,

root@debian:“# systemctl restart isc-dhcp-server.service K

root@debian: ¥
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# This declaration allows BOOTP clients to get dynamic addresses,

root@debian:“# systemctl restart isc-dhcp-server.service K

root@debian: ¥
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root@debian:“# systenctl restart isc-dhcp-server.service
root@debian:“# sustenctl status isc-dhcp-server.service
+ isc-dhcp-server.service - LSB: DHCP server
Loaded: loaded (/etc/init.dsisc-dhep-server; generated
Active: active (running) since Sun 2024-02-18 19:07:59 MSK; Imin 55 ago
Docs: man:systend-sysv-generator (8)

Process: 577 ExecStart=/etc/init.dsisc-dhep-server start (codesexited, status=0/SUCCESS
Tasks: 1 (Limit: 2315)
Hemory: 4.24
CPU: 86ms

CGroup: /system.slice/isc-dhcp-server.service
=589 susr/shinsdhepd -4 -q -cf setc/dhep/dhepd.conf enpas3

fee 18 :57 debian dhopd [586] ¢ ALL rights reserved

tes 18 57 debian dhcpd(586]: For info, please visit https://uww. isc.org/softuare/dhcp/
tes 18 57 debian dhcpd[589]: Internet Sustems Consortium DHCP Server 4.4.3-P1

tes 18 57 debian dhcpd[589]: Copuright 2004-2022 Internet Sustems Consortium

fee 18 :57 debian dhopd (5891 ALL rights reserved

fee 18 :57 debian dhcpd (5891 For info, please visit https://uwu. isc.org/softuare/dhep/
tes 18 :57 debian dhepd [589] : Wrote 0 leases to leases file

tes 18 57 debian dhcpd [S89] : Server starting service.

bes 18 59 debian isc-dhcp-server(577): Starting ISC DHCPvé server: dhepd
bes 16 19:07:59 debian systemd[1]: Started isc-dhcp-server.service - LSB: DHCP server
rootedehian:~#
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root@debian:“# systenctl restart isc-dhcp-server.service
root@debian:“# sustenctl status isc-dhcp-server.service
+ isc-dhcp-server.service - LSB: DHCP server
Loaded: loaded (/etc/init.dsisc-dhep-server; generated
Active: active (running) since Sun 2024-02-18 19:07:59 MSK; Imin 55 ago
Docs: man:systend-sysv-generator (8)

Process: 577 ExecStart=/etc/init.dsisc-dhep-server start (codesexited, status=0/SUCCESS
Tasks: 1 (Limit: 2315)
Hemory: 4.24
CPU: 86ms

CGroup: /system.slice/isc-dhcp-server.service
=589 susr/shinsdhepd -4 -q -cf setc/dhep/dhepd.conf enpas3

fee 18 :57 debian dhopd [586] ¢ ALL rights reserved

tes 18 57 debian dhcpd(586]: For info, please visit https://uww. isc.org/softuare/dhcp/
tes 18 57 debian dhcpd[589]: Internet Sustems Consortium DHCP Server 4.4.3-P1

tes 18 57 debian dhcpd[589]: Copuright 2004-2022 Internet Sustems Consortium

fee 18 :57 debian dhopd (5891 ALL rights reserved

fee 18 :57 debian dhcpd (5891 For info, please visit https://uwu. isc.org/softuare/dhep/
tes 18 :57 debian dhepd [589] : Wrote 0 leases to leases file

tes 18 57 debian dhcpd [S89] : Server starting service.

bes 18 59 debian isc-dhcp-server(577): Starting ISC DHCPvé server: dhepd
bes 16 19:07:59 debian systemd[1]: Started isc-dhcp-server.service - LSB: DHCP server
rootedehian:~#
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(a Apache2 Debian Default Page

b_

This is the default welcome page used to test the correct operation of the Apache2 server after
installation on Debian systems. If you can read this page, it means that the Apache HTTP server
installed at this site is working properly. You should replace this file (located at
/var/sau/ht)/index. hta1) before continuing to operate your HTTP server.

1f you are a normal user of this web site and don't know what this page is about, this probably means
that the site is currently unavailable due to maintenance. If the problem persists, please contact the
site's administrator.

Configuration Overview
Debian's Apache2 default configuration is different from the upstream default configuration, and split
into several files optimized for interaction with Debian tools. The configuration system is fully
documented in /usr/share/doc/apache2/README.Debian.gz. Refer to ths for the full
Gocumentation. Documentation for the web server itself can be found by accessing the manual if the
apache2-doc package was installed on ths server

‘The configuration layout for an Apache2 web server installation on Debian systems is as follows:

« apache.conf is the main configuration file. It puts the pieces together by including all remaining
configuration files when starting up the web server.

* ports.conf is always included from the main configuration file. It s used to determine the
listening ports for incoming connections, and this file can be customized anytime.
« Configuration files in the mods-enabled/, conf-enabled/ and sites-enabled/ directories contain
pariculac configuraion sngpets whch manage modides, lobelcontiurstion fragments,or vetual
‘configurations, respectively.
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(a Apache2 Debian Default Page

b_

This is the default welcome page used to test the correct operation of the Apache2 server after
installation on Debian systems. If you can read this page, it means that the Apache HTTP server
installed at this site is working properly. You should replace this file (located at
/var/sau/ht)/index. hta1) before continuing to operate your HTTP server.

1f you are a normal user of this web site and don't know what this page is about, this probably means
that the site is currently unavailable due to maintenance. If the problem persists, please contact the
site's administrator.

Configuration Overview
Debian's Apache2 default configuration is different from the upstream default configuration, and split
into several files optimized for interaction with Debian tools. The configuration system is fully
documented in /usr/share/doc/apache2/README.Debian.gz. Refer to ths for the full
Gocumentation. Documentation for the web server itself can be found by accessing the manual if the
apache2-doc package was installed on ths server

‘The configuration layout for an Apache2 web server installation on Debian systems is as follows:

« apache.conf is the main configuration file. It puts the pieces together by including all remaining
configuration files when starting up the web server.

* ports.conf is always included from the main configuration file. It s used to determine the
listening ports for incoming connections, and this file can be customized anytime.
« Configuration files in the mods-enabled/, conf-enabled/ and sites-enabled/ directories contain
pariculac configuraion sngpets whch manage modides, lobelcontiurstion fragments,or vetual
‘configurations, respectively.
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Debian GNU/Linux 12 debian ttyl

debian login: root
Passuord:
Linux debian 6.1.0-13-anded #1 SMP PREEMPT_DYNAMIC Debian 6.1.55-1 (2023-09-29) x86_64

The programs included with the Debian GNU/Linux sustem are free softuare;
the exact distribution terms for each program are described in the
individual files in /usr/share/doc/«/copuright.

Debian GNU/Linux comes with ABSOLUTELY NO HARRANTY, to the extent
permitted by applicable law.
root@dehian:“# apt update
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' FS LS SYIR 2R ATLLASYS TR/ Systol It IoHesl tal ettt Jalits/gpablioe . o5l VALE 7 722K/ Syst ol Syst ol ar
ache2.service.

Created sunlink /etc/systemd/system/multi-user.target.uants/apache-htcacheclean.service » /lib/syste
nd/systen/apache-htcacheclean. service.

OfpabaTueanTcs TpUrreps ana man-db (2.11.2-2)

0BpabaTueanTcs TpUrrep Ana mailcap (3.70+nmul)

0fpabaTueanTcs Tourreps ana libc-bin (2.36-3+deb12u3)

root@debian:™# apt install bindd isc-dhcp-server apache2 lunx nano
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' FS LS SYIR 2R ATLLASYS TR/ Systol It IoHesl tal ettt Jalits/gpablioe . o5l VALE 7 722K/ Syst ol Syst ol ar
ache2.service.

Created sunlink /etc/systemd/system/multi-user.target.uants/apache-htcacheclean.service » /lib/syste
nd/systen/apache-htcacheclean. service.

OfpabaTueanTcs TpUrreps ana man-db (2.11.2-2)

0BpabaTueanTcs TpUrrep Ana mailcap (3.70+nmul)

0fpabaTueanTcs Tourreps ana libc-bin (2.36-3+deb12u3)

root@debian:™# apt install bindd isc-dhcp-server apache2 lunx nano
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Bufop paee He BuBpaHHOrD nakeTa bind3-utils.

ToaroToska K pacnakoske ../13-bind3-utils_1%3a3.18.24-1_and64.deb
PacnakosuBaeTes bindd-utils (1:9.18.24-1

Bufiop paxee He BufpaHHoro naketa dns-root-data.

TloaroTosKka K pacnakoske ../14-dns-root-data_2023010101_all.deb
PacnakosuBaeTcs dns-root-data (2023010101

Bufop paxee He BhfpaHHOro nakeTa bind3.

ToaroToska K pacnakoske ../15-bind3_1%3a3.18.24-1_and64.deb
PacnakossBaeTes bindd (1:9.18.24-1

Bubop paHee We BwfpaHHoro nakeTa isc-dhcp-server.

ToaroToska K pacnakoske ../16-isc-dhcp-server_4.4.3-P1-2_amd6d. deb
PacnakossisaeTcs isc-dhcp-server (4.4.3-P1-2

ToaroToska K pacnakoske ../17-libcurl3-gnutls_7.88. 1- 10+deb12uS_amded. deb
PacnakosusaeTes libcurl3-gnutlsiandsd (7.88.1-10+deb12uS) Ha sameHy (7.88.1-10+debi2ud
Bufop paxee He BuBpaHHOro nakeTa lynx-common.

TloaroToska K pacnakoske ../18-lynx-common_2.3.@dev.12-1_all.deb
PacnakossaeTcs lynx-common (2.9.0dev. 1

Bufiop paree He BuOPaHHOrD nakeTa lynx.

ToaroTosxa K pacnaxoske ../13-lynx_2.9.0dev. 12-1_and64. deb
PacnakossaeTes lynx (2.3.0dev.12-1

Bufop paxee He BuBpaHHOro naketa selinux-utils.

ToaroToeka K pacnakoske ../20-selinux-utils_3.4-1+b6_andsd.deb
PacnakosuBaeTes selinux-utils (3.4-1+b6

Bufop pavee He BufpaHHoro naketa policycoreutils.

ToaroTosra K pacnaxoske ./21-policycoreutils_3.4-1_ands4.deb
PacnakosBaeTcs policucoreutils (3.4-1

Bufop paHee He BhpaHHOro naketa ssl-cert.

ToaroToska K pacnakoske ../22-ssl-cert_1.1.2_all.deb
PacnakosBaeTes ssl-cert (1.1.2

HacTpawsaeTcs nakeT selinux-utils (3.4-1+b6

HacTpaveaeTca nakeT bindg-1ibs:andsd (1:9.18.24-1

HacTpavsaeTca naket policycoreutils (3.4-1

HacTpausaeTcs naket libapriiamdsd (1.7.2-3

HacTpausaeTca naker isc-ohep-server (4.4.3-P1-2

Generating /etc/default/isc-dhcp-server. ..

X04_BbINOJHEHNS : [REBRBRERBRBRERA BB AR BB RARARARRARARARRA .
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Bufop paee He BuBpaHHOrD nakeTa bind3-utils.

ToaroToska K pacnakoske ../13-bind3-utils_1%3a3.18.24-1_and64.deb
PacnakosuBaeTes bindd-utils (1:9.18.24-1

Bufiop paxee He BufpaHHoro naketa dns-root-data.

TloaroTosKka K pacnakoske ../14-dns-root-data_2023010101_all.deb
PacnakosuBaeTcs dns-root-data (2023010101

Bufop paxee He BhfpaHHOro nakeTa bind3.

ToaroToska K pacnakoske ../15-bind3_1%3a3.18.24-1_and64.deb
PacnakossBaeTes bindd (1:9.18.24-1

Bubop paHee We BwfpaHHoro nakeTa isc-dhcp-server.

ToaroToska K pacnakoske ../16-isc-dhcp-server_4.4.3-P1-2_amd6d. deb
PacnakossisaeTcs isc-dhcp-server (4.4.3-P1-2

ToaroToska K pacnakoske ../17-libcurl3-gnutls_7.88. 1- 10+deb12uS_amded. deb
PacnakosusaeTes libcurl3-gnutlsiandsd (7.88.1-10+deb12uS) Ha sameHy (7.88.1-10+debi2ud
Bufop paxee He BuBpaHHOro nakeTa lynx-common.

TloaroToska K pacnakoske ../18-lynx-common_2.3.@dev.12-1_all.deb
PacnakossaeTcs lynx-common (2.9.0dev. 1

Bufiop paree He BuOPaHHOrD nakeTa lynx.

ToaroTosxa K pacnaxoske ../13-lynx_2.9.0dev. 12-1_and64. deb
PacnakossaeTes lynx (2.3.0dev.12-1

Bufop paxee He BuBpaHHOro naketa selinux-utils.

ToaroToeka K pacnakoske ../20-selinux-utils_3.4-1+b6_andsd.deb
PacnakosuBaeTes selinux-utils (3.4-1+b6

Bufop pavee He BufpaHHoro naketa policycoreutils.

ToaroTosra K pacnaxoske ./21-policycoreutils_3.4-1_ands4.deb
PacnakosBaeTcs policucoreutils (3.4-1

Bufop paHee He BhpaHHOro naketa ssl-cert.

ToaroToska K pacnakoske ../22-ssl-cert_1.1.2_all.deb
PacnakosBaeTes ssl-cert (1.1.2

HacTpawsaeTcs nakeT selinux-utils (3.4-1+b6

HacTpaveaeTca nakeT bindg-1ibs:andsd (1:9.18.24-1

HacTpavsaeTca naket policycoreutils (3.4-1

HacTpausaeTcs naket libapriiamdsd (1.7.2-3

HacTpausaeTca naker isc-ohep-server (4.4.3-P1-2

Generating /etc/default/isc-dhcp-server. ..

X04_BbINOJHEHNS : [REBRBRERBRBRERA BB AR BB RARARARRARARARRA .
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Debian GNU/Linux 12 debian ttyl

debian login: root
Password:
Linux debian 6.1.0-13-amd64 #1 SMP PREEMPT_DYNAMIC Debian 6.1.55-1 (2023-09-29) x86_6¢

The programs included with the Debian GNU/Linux system are free softuare;
the exact distribution terms for each program are described in the
individual files in /usr/share/doc/x/copyright.

GNU/Linux comes with ABSOLUTELY NO WARRANTY, to the extent
y applicable law.
Feb 18 15:57:19 MSK 2024 on ttyl
root@debian M ip addr
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 gdisc nogueue state UNKNOWN group default glen 1009
Link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo
valid_Lft forever preferred_Lft forever
inet6 ::1/128 scope host nopref ixroute
valid_Lft forever preferred_lft forever
2: enpos3: <BROADCAST,MULTICAST,UP,LOER_UP> mtu 1560 disc fo_codel state UP group default glen 100
o

Link/ether 08:00:27:6b:6e:3a brd ffff:ff:ffffff
inet6 fedo::a00:27ff:fech:6edas6d scope link
valid_Lft forever preferred_lft forever

root@debian:





image70.png
Debian GNU/Linux 12 debian ttyl

debian login: root
Password:
Linux debian 6.1.0-13-amd64 #1 SMP PREEMPT_DYNAMIC Debian 6.1.55-1 (2023-09-29) x86_6¢

The programs included with the Debian GNU/Linux system are free softuare;
the exact distribution terms for each program are described in the
individual files in /usr/share/doc/x/copyright.

GNU/Linux comes with ABSOLUTELY NO WARRANTY, to the extent
y applicable law.
Feb 18 15:57:19 MSK 2024 on ttyl
root@debian M ip addr
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 gdisc nogueue state UNKNOWN group default glen 1009
Link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo
valid_Lft forever preferred_Lft forever
inet6 ::1/128 scope host nopref ixroute
valid_Lft forever preferred_lft forever
2: enpos3: <BROADCAST,MULTICAST,UP,LOER_UP> mtu 1560 disc fo_codel state UP group default glen 100
o

Link/ether 08:00:27:6b:6e:3a brd ffff:ff:ffffff
inet6 fedo::a00:27ff:fech:6edas6d scope link
valid_Lft forever preferred_lft forever

root@debian:
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pebian GNU/Linux 12 debian ttyl

debian login: root
Passuord:
Linux debian 6.1.0-13-anded #1 SMP PREEMPT_DYNAMIC Debian 6.1.55-1 (2023-09-29) x86_64

The programs included with the Debian GNU/Linux sustem are free softuare;
the exact distribution terms for each program are described in the
individual files in /usr/share/doc/«/copuright.

Debian GNU/Linux comes with ABSOLUTELY NO HARRANTY, to the extent
permitted by applicable law.
Last login: Sun Feb 18 15:57:19 MSK 2024 on ttyl
root@debian:“# ip addr
lo: <LOOPBACK ,UP,LOER_UP> mtu 65536 gdisc nogueue state UNKNOWN group default glen 100
Link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo
valid_Lft forever preferred_lft forever
inet6 ::1/128 scope host nopref ixroute
valid_Lft forever preferred_lft forever
+ enpos3: <BROADCAST,MULTICAST,UP,LONER_UP> mtu 1508 qdisc fq_codel state UP group default qlen 1o

Link/ether 08:00:27:6b:6e:3a brd ffffiffiffffiff
inete feo::a00:27ff:fech:6edased scope link

valid_Lft forever preferred_lft forever
root@dehian:“# _
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pebian GNU/Linux 12 debian ttyl

debian login: root
Passuord:
Linux debian 6.1.0-13-anded #1 SMP PREEMPT_DYNAMIC Debian 6.1.55-1 (2023-09-29) x86_64

The programs included with the Debian GNU/Linux sustem are free softuare;
the exact distribution terms for each program are described in the
individual files in /usr/share/doc/«/copuright.

Debian GNU/Linux comes with ABSOLUTELY NO HARRANTY, to the extent
permitted by applicable law.
Last login: Sun Feb 18 15:57:19 MSK 2024 on ttyl
root@debian:“# ip addr
lo: <LOOPBACK ,UP,LOER_UP> mtu 65536 gdisc nogueue state UNKNOWN group default glen 100
Link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo
valid_Lft forever preferred_lft forever
inet6 ::1/128 scope host nopref ixroute
valid_Lft forever preferred_lft forever
+ enpos3: <BROADCAST,MULTICAST,UP,LONER_UP> mtu 1508 qdisc fq_codel state UP group default qlen 1o

Link/ether 08:00:27:6b:6e:3a brd ffffiffiffffiff
inete feo::a00:27ff:fech:6edased scope link

valid_Lft forever preferred_lft forever
root@dehian:“# _
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# This file describes the network interfaces available on your system
# and how to activate them. For more information, see interfaces(s).

source /etc/netuork/ interfaces.d/x

# The loopback netuork interface
auto lo
iface lo inet loophack

# The primary network interface
allou-hotplug enpasa
iface enpos3 inet dhcp
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# This file describes the network interfaces available on your system
# and how to activate them. For more information, see interfaces(s).

source /etc/netuork/ interfaces.d/x

# The loopback netuork interface
auto lo
iface lo inet loophack

# The primary network interface
allou-hotplug enpasa
iface enpos3 inet dhcp

Crpaska
BbiX0A

3anucats Touck
UnTiain amera

Bbipesars
il GcrasuTe

BHNOAHNTE
BPOBHATE

Tosnuus
K cTpoke

OTHEHa
ToeTop




image10.png
# This file describes the network interfaces available on your system
# and how to activate them. For more information, see interfaces(s).

source /etc/network/ interfaces.d/x

# The loopback netuork interface
auto lo
iface lo inet loophack

# The primary network interface

allou-hotplug enpasa

iface enpos3 inet static
address 192.168.10. 1
netmask 255.255.255.0
gateway 192.166.10. 1
dns-namesevers 192.168.10.1
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# This file describes the network interfaces available on your system
# and how to activate them. For more information, see interfaces(s).

source /etc/network/ interfaces.d/x

# The loopback netuork interface
auto lo
iface lo inet loophack

# The primary network interface

allou-hotplug enpasa

iface enpos3 inet static
address 192.168.10. 1
netmask 255.255.255.0
gateway 192.166.10. 1
dns-namesevers 192.168.10.1
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-ootadebian: “# systemctl restart networking.service
ootadebian:™# ip addr
11 lo: <LDOPBACK,UP,LOWER_UP> mtu 65536 gdisc nogueue state UNKNOWN group default olen 1000
Link/loopback 00:00:00:00:00:00 hrd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo
valid_Lft forever preferred_lft forever
inet6 ::1/128 scope host nopref ixrol
valid_Lft forever preferre
enpos3: <BROADCAST, MULT,

Link/ether 88:00:27:6h:08: BARAERs” (hat]

inet 132.166.10.1/24 brd 192.168.10.255 s:ﬂb
valid_Lft forever preferred_Lft forever

inet6 fedo::a00:27ff:fechite3a/ed scope link

valid_Lft forever preferred_lft forever
oot@dehian: ~#

KER_UP> mtu 1560 gdisc fo_codel state UP group default glen 1o
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-ootadebian: “# systemctl restart networking.service
ootadebian:™# ip addr
11 lo: <LDOPBACK,UP,LOWER_UP> mtu 65536 gdisc nogueue state UNKNOWN group default olen 1000
Link/loopback 00:00:00:00:00:00 hrd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo
valid_Lft forever preferred_lft forever
inet6 ::1/128 scope host nopref ixrol
valid_Lft forever preferre
enpos3: <BROADCAST, MULT,

Link/ether 88:00:27:6h:08: BARAERs” (hat]

inet 132.166.10.1/24 brd 192.168.10.255 s:ﬂb
valid_Lft forever preferred_Lft forever

inet6 fedo::a00:27ff:fechite3a/ed scope link

valid_Lft forever preferred_lft forever
oot@dehian: ~#

KER_UP> mtu 1560 gdisc fo_codel state UP group default glen 1o
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root@debian:“# systemctl restart networking.service
root@debian:“# ip addr
1t lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc nogueue state UNKNOWN group default glen 1000
Link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo
valid_lft forever preferred_lft forever
ineté ::1/128 scope host nopref ixroute
valid_lft forever preferred_lft forever
2t enpos3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fo_codel state UP group default glen 10
0

link/ether 08:00:27:6b:6e:3a brd ff:ff:ff:ff:ff:ff
inet 192.168.10.1/24 brd 792.168.10.255 scope global enposd
valid_lft forever preferred_lft forever
inet feo::a00:27ff:fed:fedas6d scope link
valid_Lft forever piWferred_Lft forever
rootadebian:“# ping 192.166.10.1
PING 192.168.10.1 (192.168.10.1) 56(84) bytes of data

64 bytes from 192.168.10.1: icmp_seq=1 ttl=6d tine=0.050 ns
64 bytes from 192.168.10.1: icip_seq=2 ttl=6d tine=0.068 ns
64 bytes from 192.168.10.1: icip_seq=3 ttl=6d tine=0.062 ns
64 bytes from 192.168.10.1: icmp_seq=d ttl=6d tine=0.063 ns
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root@debian:“# systemctl restart networking.service
root@debian:“# ip addr
1t lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc nogueue state UNKNOWN group default glen 1000
Link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo
valid_lft forever preferred_lft forever
ineté ::1/128 scope host nopref ixroute
valid_lft forever preferred_lft forever
2t enpos3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fo_codel state UP group default glen 10
0

link/ether 08:00:27:6b:6e:3a brd ff:ff:ff:ff:ff:ff
inet 192.168.10.1/24 brd 792.168.10.255 scope global enposd
valid_lft forever preferred_lft forever
inet feo::a00:27ff:fed:fedas6d scope link
valid_Lft forever piWferred_Lft forever
rootadebian:“# ping 192.166.10.1
PING 192.168.10.1 (192.168.10.1) 56(84) bytes of data

64 bytes from 192.168.10.1: icmp_seq=1 ttl=6d tine=0.050 ns
64 bytes from 192.168.10.1: icip_seq=2 ttl=6d tine=0.068 ns
64 bytes from 192.168.10.1: icip_seq=3 ttl=6d tine=0.062 ns
64 bytes from 192.168.10.1: icmp_seq=d ttl=6d tine=0.063 ns
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64 butes from 192.168.10.1

"2
[1]+ OcTaHonen  ping 192.168. 1
root@debian:~# ls /var/uwu/htnl/

index. htnl
root@debian:“#
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64 butes from 192.168.10.1

"2
[1]+ OcTaHonen  ping 192.168. 1
root@debian:~# ls /var/uwu/htnl/

index. htnl
root@debian:“#
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[1]+ OcTaHoBned  ping 132.168.10.1

-ootadebian:™# s /var/wwhinl/
index. html /
-ootadebian:“# s /etc/apaches/

pachez.conf  conf-enabled nagic nods-enabled  sites-available
onf-available enwars nods-available ports.conf  sites-enabled
ontadehian: “# -
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[1]+ OcTaHoBned  ping 132.168.10.1

-ootadebian:™# s /var/wwhinl/
index. html /
-ootadebian:“# s /etc/apaches/

pachez.conf  conf-enabled nagic nods-enabled  sites-available
onf-available enwars nods-available ports.conf  sites-enabled
ontadehian: “# -
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# cd /etc/apachez/sites-available
etc/apache2/sites-availabled
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# cd /etc/apachez/sites-available
etc/apache2/sites-availabled
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<Virtuallost *:80>
serverianme nad.ex
serverfdnin admingnad. ex
DocumentRoot /var/uu/nad/
</VirtualHost>
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<Virtuallost *:80>
serverianme nad.ex
serverfdnin admingnad. ex
DocumentRoot /var/uu/nad/
</VirtualHost>
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/

etc/apache2/sites-available# mkdir /var/wuw/mad
i/etc/apache2/sites-available# 1s svar/uwu/

wtml  nad

etc/apache2/sites-available# _
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/

etc/apache2/sites-available# mkdir /var/wuw/mad
i/etc/apache2/sites-available# 1s svar/uwu/

wtml  nad

etc/apache2/sites-available# _
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root@debian: /etc/apaches/s ites-avallables mkdir /var/ww/nad
rootadebian: /ete/apachez/s ites-avallables 1s /var/uuw/

html  na3
root@debian: /etc/apache2/sites-available# cd
root cd /etc/apache2/sites-available
root@debian sites-available# cd ..
root@debian: /etc/apal ls

apache2.conf conf-efiabled magic mods-enabled sites-available
conf-available envvars mods-available ports.conf sites-enabled
root@debian: /etc/apache2# ls sites-available

000-default.conf default-ssl.conf nad.ex.conf

root@debian: /etc/apache2#
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root@debian: /etc/apaches/s ites-avallables mkdir /var/ww/nad
rootadebian: /ete/apachez/s ites-avallables 1s /var/uuw/

html  na3
root@debian: /etc/apache2/sites-available# cd
root cd /etc/apache2/sites-available
root@debian sites-available# cd ..
root@debian: /etc/apal ls

apache2.conf conf-efiabled magic mods-enabled sites-available
conf-available envvars mods-available ports.conf sites-enabled
root@debian: /etc/apache2# ls sites-available

000-default.conf default-ssl.conf nad.ex.conf

root@debian: /etc/apache2#
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root@debian:/etc/apachee/sites-available# mkdir /var/uuw/nad
root@debian:/etc/apachee/sites-available# s /var/wuu/
html na3
root@debian:/etc/apachea/sites-available# cd
root@debian:“# cd /etc/apache2/sites-avallab
root@debian:/etc/apaches/sites-availables
root@dehian:/etc/apachezd ls
apachez.conf  conf-enabled magic
conf-available envvars mods-
root@debian:/etc/apachee# s site) ilable
000-default.conf default-ssl.cor a3, ex.conf
root@debian:/etc/apache2# azensite na3.ex.conf
Enabling site na3.ex.
To activate the new configuration, you need to run:
systemctl reload apachez
root@debian:/etc/apache2#

mods-enabled sites-available
able ports.conf  sites-enabled
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root@debian:/etc/apachee/sites-available# mkdir /var/uuw/nad
root@debian:/etc/apachee/sites-available# s /var/wuu/
html na3
root@debian:/etc/apachea/sites-available# cd
root@debian:“# cd /etc/apache2/sites-avallab
root@debian:/etc/apaches/sites-availables
root@dehian:/etc/apachezd ls
apachez.conf  conf-enabled magic
conf-available envvars mods-
root@debian:/etc/apachee# s site) ilable
000-default.conf default-ssl.cor a3, ex.conf
root@debian:/etc/apache2# azensite na3.ex.conf
Enabling site na3.ex.
To activate the new configuration, you need to run:
systemctl reload apachez
root@debian:/etc/apache2#

mods-enabled sites-available
able ports.conf  sites-enabled
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root@debian:/etc/apachee/sites-availabled mkdir /var/uuw/nas

root@debian:/etc/apachee/sites-available# s /var/wu/

html na3

root@debian:/etc/apachez/sites-available# cd

root@debian:“# cd /etc/apache2/sites-available

root@debian:/etc/apachea/sites-available# cd .

root@dehian: /etc/apachezt s

apachez.conf  conf-enabled magic mods-enabled

conf-available envvars mods-available ports.con

root@debian:/etc/apachee# s sites-available

000-default.conf default-ssl.conf nad.ex.con

root@debian:/etc/apache2# azensite nad.ex.conf

Enabling site nad.ex.

To activate the new configuration, you need to run:
systemctl reload apachez

root@debian:/etc/apachee# systemctl reload apache2.service

root@debian: /etc/apache2# _

sites-available
sites-enabled
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root@debian:/etc/apachee/sites-availabled mkdir /var/uuw/nas

root@debian:/etc/apachee/sites-available# s /var/wu/

html na3

root@debian:/etc/apachez/sites-available# cd

root@debian:“# cd /etc/apache2/sites-available

root@debian:/etc/apachea/sites-available# cd .

root@dehian: /etc/apachezt s

apachez.conf  conf-enabled magic mods-enabled

conf-available envvars mods-available ports.con

root@debian:/etc/apachee# s sites-available

000-default.conf default-ssl.conf nad.ex.con

root@debian:/etc/apache2# azensite nad.ex.conf

Enabling site nad.ex.

To activate the new configuration, you need to run:
systemctl reload apachez

root@debian:/etc/apachee# systemctl reload apache2.service

root@debian: /etc/apache2# _

sites-available
sites-enabled
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‘oot@debian:/etc/apachee# ls sites-available

00-default.conf default-ssl.conf nad.ex.cor
oot@debian: /etc/apachez# 1s sites-enabled
00-default.conf nad.ex.conf

-ootadebian: /etc/apache2y
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‘oot@debian:/etc/apachee# ls sites-available

00-default.conf default-ssl.conf nad.ex.cor
oot@debian: /etc/apachez# 1s sites-enabled
00-default.conf nad.ex.conf

-ootadebian: /etc/apache2y
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IaeT nouCK nad.ex_cHauana
0T NOWCK Wy.Na3 . £X.COM, UragHBaHie.
0eT NOWCK Wuw.nad. ex. edu, UraneaHie
0eT NOWCK Ww.Na3.ex.net, UraneaHie
0eT NOWCK Wy.Na3.EX.0rg, UrankBaHie
feT aocTyna file://localhost/etc/apachez/nad.ex’
HAMaHVE |1 DWMBKa AOCTUNE K ADKYMEHTY

lynx: HET ADCTYNA K HauanbHoMy dainy
‘oot@debian: /etc/apachesd
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IaeT nouCK nad.ex_cHauana
0T NOWCK Wy.Na3 . £X.COM, UragHBaHie.
0eT NOWCK Wuw.nad. ex. edu, UraneaHie
0eT NOWCK Ww.Na3.ex.net, UraneaHie
0eT NOWCK Wy.Na3.EX.0rg, UrankBaHie
feT aocTyna file://localhost/etc/apachez/nad.ex’
HAMaHVE |1 DWMBKa AOCTUNE K ADKYMEHTY

lynx: HET ADCTYNA K HauanbHoMy dainy
‘oot@debian: /etc/apachesd
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S Hem T e e AT s e e e e e e

HuMaHne | : Dwnfika AOCTUNG K AOKYMEHTY

lunx: HET ADCTYNG K HAuanbHOMy daitny
-ootadebian: /etc/apachee# nano /etc/hosts
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S Hem T e e AT s e e e e e e

HuMaHne | : Dwnfika AOCTUNG K AOKYMEHTY

lunx: HET ADCTYNG K HAuanbHOMy daitny
-ootadebian: /etc/apachee# nano /etc/hosts
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ollowing lines are
localhost ips-localhost ip6-loopl

t:1 ip6-allnodes

2 ips-allrouters

capable hosts
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[2]+ OcTaWoenew  lunx nad.ex

root@debian: /etc/apache2# > /var/wuw/mad/ex. tx
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0 CCHAKE; BAEBO - BOSBPAT.
ok [delete] =cnucok weTopun
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[2]+ OcTaWoenew  lunx nad.ex

root@debian: /etc/apache2# > /var/wuw/mad/ex. tx
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0 CCHAKE; BAEBO - BOSBPAT.
ok [delete] =cnucok weTopun
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127.0.0.1 localhost
127.0.1. debian

#127.0.0.1 nad.ex

# The following lines are Wesiral

localhost ips-localhost ips-loopback
1 ipe-allnodes

2 ips-allrouters
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# The following lines are Wesiral

localhost ips-localhost ips-loopback
1 ipe-allnodes

2 ips-allrouters
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etc/apachezd cd /
# cd setc/bind/

etc/bind# 1s

ind.keys db.127 db.empty named.conf named.conf. local rndc. key
.o db.2s5 db.local named.conf.default-zones named.conf.options zones.rfcl9ig
aot@debian: /ete/bindy
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etc/apachezd cd /
# cd setc/bind/

etc/bind# 1s

ind.keys db.127 db.empty named.conf named.conf. local rndc. key
.o db.2s5 db.local named.conf.default-zones named.conf.options zones.rfcl9ig
aot@debian: /ete/bindy
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-ootadehian: /etc/apache2# cd

ootadebian:“# cd /etc/bind/

-ootadebian: /etc/bind# ls

ind.keys db.127 db.emnty named.conf named.conf.local  rndc.key
.o db.255 db.local named.conf.@Eault-zones named.conf.options zones.ric191s

-oot@debian:/etcs/bind# nano named.conf.options
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-ootadehian: /etc/apache2# cd

ootadebian:“# cd /etc/bind/

-ootadebian: /etc/bind# ls

ind.keys db.127 db.emnty named.conf named.conf.local  rndc.key
.o db.255 db.local named.conf.@Eault-zones named.conf.options zones.ric191s

-oot@debian:/etcs/bind# nano named.conf.options
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antions {

directory "svar/cache/bind"

/¢ 1f there is a firewall betueen you and nameservers you want
/¢ to talk to, you may need to fix the firewall to allow multiple
/¢ ports to talk. See http://www.kb.cert.org/vuls/id/800113

/¢ 1f your ISP provided one or more IP addresses for stable

// nameservers, you probably want to use them as foruarders.

/7 Uncomnent the following block, and insert the addresses replacing
/¢ the all-e's placeholder.

/¢ foruarders {
0 0.0.0.0
8t

/1
// 1f BIND logs error messages about the root key being expired

// you will need to update your keys. See https://www.isc.org/bind-keys
/1
dnssec-validation auto;

listen-on-vée { any; };

OTMEHa
ToBTOp

Bbipesarh
BCTaBUTH

3anucats Towck
YaTann JaMeHa

BHNOAHNTE Tosnuus
BHPOBHATE K cTpoke

Crpaska
BbIXOA
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antions {

directory "svar/cache/bind"

/¢ 1f there is a firewall betueen you and nameservers you want
/¢ to talk to, you may need to fix the firewall to allow multiple
/¢ ports to talk. See http://www.kb.cert.org/vuls/id/800113

/¢ 1f your ISP provided one or more IP addresses for stable

// nameservers, you probably want to use them as foruarders.

/7 Uncomnent the following block, and insert the addresses replacing
/¢ the all-e's placeholder.

/¢ foruarders {
0 0.0.0.0
8t

/1
// 1f BIND logs error messages about the root key being expired

// you will need to update your keys. See https://www.isc.org/bind-keys
/1
dnssec-validation auto;

listen-on-vée { any; };
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Crpaska
BbIXOA





image33.png
acl munetuork {192.168.10.0/24; 127.0.0.1;15
options {
directory "/var/cache/bind";

\fnr‘mader‘s 18.5.8.851

/ If there is a firewall betueen you and nameservers you want
// to talk to, you may need to fix the firewall to allow multiple
/¢ ports to talk. See http://uww.kb.cert.org/vuls/id/800113

Crpaska
Bbixoa

/¢ 1f your ISP provided one or more IP addresses for stable

/¢ nameservers, you probably want to use them as foruarders.

/¢ Uncomnent the following block, and insert the addresses replacing
/¢ the all-g's placeholder.

/¢ foruarders {
20 0.0.0.0

at

listen-on {
192.168.10.1

}

/7=

// 1f BIND logs error messages about the root key being expired

// you will need to update your keys. See https://www.isc.org/bind-keys
/
dnssec-validation auto;
auth-nxdomain no;
allou-guery {mynetuork;}

~

3anucats Towck Bbpesats BHINOHATE Tosnuus
UnTBain 3ameHa BCTaBUTL BLpOBHATE [

listen-on-vé6 { none; };

OTHEHa
TiosTop
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acl munetuork {192.168.10.0/24; 127.0.0.1;15
options {
directory "/var/cache/bind";

\fnr‘mader‘s 18.5.8.851

/ If there is a firewall betueen you and nameservers you want
// to talk to, you may need to fix the firewall to allow multiple
/¢ ports to talk. See http://uww.kb.cert.org/vuls/id/800113

Crpaska
Bbixoa

/¢ 1f your ISP provided one or more IP addresses for stable

/¢ nameservers, you probably want to use them as foruarders.

/¢ Uncomnent the following block, and insert the addresses replacing
/¢ the all-g's placeholder.

/¢ foruarders {
20 0.0.0.0

at

listen-on {
192.168.10.1

}

/7=

// 1f BIND logs error messages about the root key being expired

// you will need to update your keys. See https://www.isc.org/bind-keys
/
dnssec-validation auto;
auth-nxdomain no;
allou-guery {mynetuork;}

~

3anucats Towck Bbpesats BHINOHATE Tosnuus
UnTBain 3ameHa BCTaBUTL BLpOBHATE [

listen-on-vé6 { none; };

OTHEHa
TiosTop





image34.png
‘oot@debian:/etc/bind# named-checkconf
‘etc/bind/named.conf.options:26: missing ';' before 'dnssec-validation' N
retc/bind/named.conf.options:30: missing ';' before 'listen-on-ve'

ootadehian: setc/bind# \
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‘oot@debian:/etc/bind# named-checkconf
‘etc/bind/named.conf.options:26: missing ';' before 'dnssec-validation' N
retc/bind/named.conf.options:30: missing ';' before 'listen-on-ve'

ootadehian: setc/bind# \
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acl munetuork {132.168.10.0/2
options {
directory "/var/cache/bind";

127.0.0.15}

//foruaders {8.8.8.8;};

/¢ 1f there is a firewall betueen you and nameservers you want
/¢ to talk to, you may need to fix the firewall to allow multiple
/¢ ports to talk. See http://uww.kb.cert.org/vuls/id/800113

/¢ 1f your ISP provided one or more IP addresses for stable

/¢ nameservers, you probably want to use them as foruarders.

/¢ Uncomnent the following block, and insert the addresses replacing
/¢ the all-a's placeholder.

/¢ foruarders {
0.0.0.0;

isten-on {
192.168.10.1;

// 1f BIND logs error messages about the root key being expired

// you will need to update your keys. See https://www.isc.org/bind-keys
14
dnssec-validation auto;
auth-nxdomain no;
allou-guery {mynetwork;}

listen-on-vé { none; };
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YaTdann JaMeHa

OTHEHa
ToBTOp
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acl munetuork {132.168.10.0/2
options {
directory "/var/cache/bind";

127.0.0.15}

//foruaders {8.8.8.8;};

/¢ 1f there is a firewall betueen you and nameservers you want
/¢ to talk to, you may need to fix the firewall to allow multiple
/¢ ports to talk. See http://uww.kb.cert.org/vuls/id/800113

/¢ 1f your ISP provided one or more IP addresses for stable

/¢ nameservers, you probably want to use them as foruarders.

/¢ Uncomnent the following block, and insert the addresses replacing
/¢ the all-a's placeholder.

/¢ foruarders {
0.0.0.0;

isten-on {
192.168.10.1;

// 1f BIND logs error messages about the root key being expired

// you will need to update your keys. See https://www.isc.org/bind-keys
14
dnssec-validation auto;
auth-nxdomain no;
allou-guery {mynetwork;}

listen-on-vé { none; };
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'’
// Do any local configuration here
/"

// Consider adding the 1918 zones here, if they are not used in your
// organization
//include "vetc/bind/zones.rfe1918";

zone "ex" {
tupe master;
file "setc/bind/fz_ex";

zone "'10.168.192. in-addr.arpa”{
tupe master;
file "etc/bind/rz_ex's

root@debian: /etc/bind# named-checkconf
root@debian: /etc/bindd
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'’
// Do any local configuration here
/"

// Consider adding the 1918 zones here, if they are not used in your
// organization
//include "vetc/bind/zones.rfe1918";

zone "ex" {
tupe master;
file "setc/bind/fz_ex";

zone "'10.168.192. in-addr.arpa”{
tupe master;
file "etc/bind/rz_ex's

root@debian: /etc/bind# named-checkconf
root@debian: /etc/bindd




image37.png
root@debian:/etc/bind# named-checkconf
root@dehian:/etc/bind# cat dh.local

; BIND data file for local loopback interface

STTL 604800

@ ™ S0 localhost. root.localhost.
2 3 serial
604808 ; Refresh
86400 3 Retry
2413200 ; Expire
604808 ) ; Negative Cache TTL
@ ™ NS localhost.
] N A 127.0.0.1
] N ARAR 1

rootadebian: setc/bind# cp db, local fz_ex
root@debian:/etc/bindd nano fz_ex_ -
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root@debian:/etc/bind# named-checkconf
root@dehian:/etc/bind# cat dh.local

; BIND data file for local loopback interface

STTL 604800

@ ™ S0 localhost. root.localhost.
2 3 serial
604808 ; Refresh
86400 3 Retry
2413200 ; Expire
604808 ) ; Negative Cache TTL
@ ™ NS localhost.
] N A 127.0.0.1
] N ARAR 1

rootadebian: setc/bind# cp db, local fz_ex
root@debian:/etc/bindd nano fz_ex_ -
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; BIND data file for local loopback interface

'

STTL 604801

SORIGIN ex.
@ N

N
IN
IN
IN
N

S0A www adnin (
_ap 2024021801 ; Serial
604800 3 Refresh
86400 3 Retry
2413200 3 Expire
604800 ) 3 Negative Cache TTL
NS . ex.
A 192.168.10.1 *—
A 192.168.10.1
A 192.168.10.1
A 192.168.10.1_
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; BIND data file for local loopback interface

'

STTL 604801

SORIGIN ex.
@ N

N
IN
IN
IN
N

S0A www adnin (
_ap 2024021801 ; Serial
604800 3 Refresh
86400 3 Retry
2413200 3 Expire
604800 ) 3 Negative Cache TTL
NS . ex.
A 192.168.10.1 *—
A 192.168.10.1
A 192.168.10.1
A 192.168.10.1_
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; BIND data file for local loopback interface

STTL 604800
SORIGIN ex.
@ N

IN
IN
IN
IN
IN

root@debian: /etc/bind# cp fz_ex rz_ex

S0A

wo adn.
2024021
604800

86400
2419200
604800

. ex.
192,168
192,168
192,168
192,168

in €
801

10,1
.10.1
.10.1
10,1

; serial
Refresh
Retry
Expire
Negative Cache TTL
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; BIND data file for local loopback interface

STTL 604800
SORIGIN ex.
@ N

IN
IN
IN
IN
IN

root@debian: /etc/bind# cp fz_ex rz_ex

S0A
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2024021
604800

86400
2419200
604800

. ex.
192,168
192,168
192,168
192,168

in €
801

10,1
.10.1
.10.1
10,1

; serial
Refresh
Retry
Expire
Negative Cache TTL
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; BIND data file for local loopback interface

STTL 604800

SORIGIN 10.168.192. in-addr.arpa.
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; BIND data file for local loopback interface
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rootadebian: /etc/hinde /
rootedebian: setc/bind# systenctl restart bindd_
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rootadebian: /etc/hinde /
rootedebian: setc/bind# systenctl restart bindd_
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root@debian: /etc/bindd

rootedebian: /etc/bind# systemctl restart binds
rootadebian: /etc/bind# systemctl status bindd
o named.service - BIND Domain Name Server

Loaded: loaded (/1ibssystend/systen/naned.service; enabled; preset: enabled

Active
Docs

Main PID: 915 (named)

Status: "running”
Tasks: 4 (Limit:
Memory: 18.2H

CPU: 205mS

2315)

active (running) since Sun 2024-02-18 18
man:named (8)

CGroup: /system.slice/named.service
=915 susr/shin/naned -f -u bind
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org/AARA/IN': 2}
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root@debian: /etc/bindd

rootedebian: /etc/bind# systemctl restart binds
rootadebian: /etc/bind# systemctl status bindd
o named.service - BIND Domain Name Server

Loaded: loaded (/1ibssystend/systen/naned.service; enabled; preset: enabled

Active
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root@debian: /etc/bind# named-checkconf -z

zone ex/IN: loaded serial 2024621801

zone 10.168.192. in-addr.arpa/IN: loaded serial 2024621801
zone localhost/IN: loaded serial 2

zone 127.in-addr.arpa/IN: loaded serial 1

zone ©.in-addr.arpa/IN: loaded serial 1

zone 255. in-addr.arpa/IN: loaded serial 1

root@debian: /etc/bind#
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BbIX0A

ECTb OCTAHOBAEHHHE SAAHNA .

root@debian: /etc/bind# named-checkconf -z
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